This project is heavily based on the similar one by Martin Thomas. 
It creates a virtual COM port (the requred driver is in the drv_inf directory) 
and bridges it to RS232_0 on the board. The serial port speed is defined in interrupt_Usart.c 
and is set to 115200 by default.