Projects for STR7 boards use following external tools: 

1. OpenOCD STR7 - this tool is used to start connection to STR7 board. To add this external tool goto "Run->External tools->Open external tools dialog". Now click on Program and then on New button.
 This way you will create configuration with selected type. 
	You have to fill the External Tools window this way:

		o) In the Name textbox insert: OpenOCD STR7
		o) In the Location textbox insert the path of the OpenOCD executable. Using "Browse File System… " option it’s possible to find this file location,
		 that on MS Windows should be -  C:\gccfd\openocd\bin\openocd-ftd2xx.exe
		o) In the Working Directory textbox insert the path of the folder openocd­configs. In our case : ${project_loc}
		o) In the Arguments  textbox insert the option:  -f ${project_loc}\armusbocd.cfg 


2. OpenOCD STR7 Erase - this tool is used to erase STR7 internal Flash. To add this external tool goto "Run->External tools->Open external tools dialog". Now click on Program and then on New button.
 This way you will create configuration with selected type. 
	You have to fill the External Tools window this way:

		o) In the Name textbox insert: OpenOCD STR7 Erase 
		o) In the Location textbox insert the path of the OpenOCD executable. Using "Browse File System…" option it’s possible to find this file location,
		 that on MS Windows should be -  C:\gccfd\openocd\bin\openocd-ftd2xx.exe
		o) In the Working Directory textbox insert the path of the folder openocd­configs. In our case : ${project_loc}
		o) In the Arguments  textbox insert the option: -f ${project_loc}\armusbocd-flash-erase.cfg


3. OpenOCD STR7 Program - this tool is used to program STR7 internal Flash. To add this external tool goto "Run->External tools->Open external tools dialog". Now click on Program and then on New button.
 This way you will create configuration with selected type. 
	You have to fill the External Tools window this way:

		o) In the Name textbox insert: OpenOCD STR7 Program
		o) In the Location textbox insert the path of the OpenOCD executable. Using "Browse File System…" option it’s possible to find this file location,
		 that on MS Windows should be -  C:\gccfd\openocd\bin\openocd-ftd2xx.exe
		o) In the Working Directory textbox insert the path of the folder openocd­configs. In our case : ${project_loc}
		o) In the Arguments  textbox insert the option: -f ${project_loc}\armusbocd-flash-program.cfg 